- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tail Gate / Tail Gate Assembly Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Tail Gate / Tail Gate Assembly Repair procedures

Replacement

• | Wear gloves to protect hands from injury.

• | When removing and installing the tail gate, work in a group of two or more.

1. | Remove the tail gate trim. (Refer to Tail Gate - "Tail Gate Trim")

2. | Disconnect the washer nozzle hose (A).

3. | Disconnect the connectors (A) and tail gate wiring harness (B).

4. | Loosen the ground bolts (C).

5. | After loosening the mounting bolts, remove the tail gate assembly (D).
Tightening torque : 21.6~26.5 N.m (2.2~2.7 kgf.m, 15.9~19.5 lb-ft)

6. | Using a screwdriver, lift the socket clips (A) up slightly on both ends of the tail gate lifter (B).

7. | Install in the reverse order of removal.
• | Make sure that the tail gate locks/unlocks and opens/closes properly.
• | Adjust the tail gate alignment.
• | Make sure that the connectors are connected properly.
• | Replace any damaged clips.

##### Tail Gate Assembly Components and Components Location

Component Location 1. Tail gate assembly ...

##### Tail Gate Trim Components and Components Location

Component Location 1. Tail gate trim ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Belt Retractor Repair procedures

Replacement • When installing the belt, be careful not to damage the retractor. 1. Remove the rear pillar trim. (Refer to Interior Trim - "Rear Pillar Trim") 2. Loosen the rear seat belt upper anchor (A) mounting bolt. 3. After loosening the ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Brake Bleeding Prcoedure

AHB Brake System Bleeding procedure • Do not reuse the drained fluid.. • Always use genuine DOT3/DOT4 brake fluid. Using a non-genuine DOT3/DOT4 brake fluid can cause corrosion and decrease the life of the system. • Make sure no di ...
Copyright © www.ksoulev.com 2020-2021