- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Power Windows / Power Window Relay Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Power Windows / Power Window Relay Repair procedures

Inspection

Diagnosis With GDS

1. | It can quickly diagnose defects of power window by communicating with GDS. GDS can operate actuator forcefully, monitor input/output values and self diagnose.

2. | Select model and "BCM".

3. | Select the "SJB" to check.

4. | Select "Current Data" if you wish to check the current data of power window system. This menu provides input/output status of SJB.

5. | If you wish to check the power door lock operation forcefully, select "Actuation test".

##### Power Window Switch Repair procedures

Inspection Power Window Main Switch Inspection 1. Disconnect the negative (-) battery terminal. 2. Remove the front door trim. (Refer to Body - "Front Door Trim") 3. Disconnect the conne ...

##### Rear Glass Defogger

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Power Window Switch Components and Components Location

Components Driver Power Window Switch Assist Power Window Switch Rear Power Window Switch ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Repair procedures

Inspection Battery Voltage and Status Check the battery voltage and status using the battery tester. Battery Terminal 1. Move back and forth to check that the battery terminals (A) are loose or corroded. If the terminals are corroded, clean them. If battery posi ...
Copyright © www.ksoulev.com 2020-2021