- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Steering wheel / Heated Steering wheel Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Steering System / Steering wheel / Heated Steering wheel Description and Operation

Description

When manually selected, the heated steering wheel system improves the thermal comfort of the driver by heating the steering wheel.

1. | Heate control unit

2. | Heated pad Specifications
Item | Specification
standard | minimum | maximum
Voltage | 13.5 V | 9 V | 16 V
Heated pad resistance | 1.73? | 1.56? | 1.90?
NTC resistance | 10.0 k? | 9k? | 11k?

##### Repair procedures

Replacement 1. Disconnect the battery negative cable from the battery and then wait for at least 30 seconds. 2. Turn the steering wheel so that the front wheels are facing straight ahead. 3 ...

##### Heated Steering wheel Schematic Diagrams

System Circuit Diagram ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Disc Brake Components and Components Location

Components 1. Guide rod bolt2. Bleed screw3. Caliper carrier4. Caliper body5. Brake pad6. Pad retainer ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Side Weatherstrip Repair procedures

Replacement 1. Loosen the rear door checker (B) mounting bolt. Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m, 12.3 ~ 15.9 lb-ft) 2. Detach the clips, then remove the rear door side weatherstrip (A). 3. Install in the reverse order of removal. ...
Copyright © www.ksoulev.com 2020-2021