- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / Schematic Diagrams

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / Schematic Diagrams

Circuit Diagram (1)

Circuit Diagram (2)

Circuit Diagram (3)

SRSCM Connector Terminal

Harness Connector

Pin No. | Function (Connector A) | Pin No. | Function (Connector B)
1 | - | - | 1 | - | -
2 | - | - | 2 | - | -
3 | - | - | 3 | - | -
4 | - | - | 4 | - | -
5 | G | A/C Control Module (SBR PASS) | 5 | B | Passenger Side Impact Sensor (High)
6 | - | - | 6 | Y | Passenger Side Impact Sensor (Low)
7 | P | Smart Junction Box(Fuse - AIR BAG) | 7 | O | Driver Side Impact Sensor (Low)
8 | R | Driver Front Impact Sensor (High) | 8 | G | Driver Side Impact Sensor (High)
9 | L | Driver Front Impact Sensor (Low) | 9 | - | -
10 | G | Passenger Front Impact Sensor (Low) | 10 | B | Ground (GF07)
11 | O | Passenger Front Impact Sensor (High) | 11 | - | -
12 | - | - | 12 | Gr | Driver Side Air Bag (High)
13 | - | - | 13 | W/B | Driver Side Air Bag (Low)
14 | - | - | 14 | P/B | Passenger Side Air Bag (Low)
15 | - | - | 15 | O/B | Passenger Side Air Bag (High)
16 | - | - | 16 | - | -
17 | - | - | 17 | - | -
18 | - | - | 18 | - | -
19 | - | - | 19 | - | -
20 | - | - | 20 | - |
21 | - | - | 21 | R | Passenger Pressure Side Impact Sensor (Low)
22 | - | - | 22 | L | Passenger Pressure Side Passenger Pressure Side
23 | - | - | 23 | B | Driver Curtain Air Bag (High)
24 | - | - | 24 | R | Driver Curtain Air Bag (Low)
25 | Gr | Passenger Air Bag #3 (Low) | 25 | Y | Passenger Curtain Aig Bag (Low)
26 | Y | Passenger Air Bag #3 (High) | 26 | W | Passenger Curtain Aig Bag (High)
27 | - | - | 27 | - | -
28 | - | - | 28 | - | -
29 | - | - | 29 | - | -
30 | - | - | 30 | - | -
31 | - | - | 31 | G | Passenger Seat Balt Buckle Switch (+)
32 | Br | Integrated Brake Actuation Unit (Local CAN Low) | 32 | B/O | Driver Seat Belt Buckle Switch (+)
33 | G | Integrated Brake Actuation Unit (Local CAN High) | 33 | B | Driver Seat Belt Buckle Switch (-)-
34 | O | Crash Output | 34 | L | Driver Anchor Pretensioner (High)
35 | G | Driver Air Bag (2nd Satge (Low)) | 35 | Br | Driver Anchor Pretensioner (Low)
36 | O | Driver Air Bag (2nd Satge (High)) | 36 | Y | Passenger Anchor Pretensioner(Low)
37 | W | Passenger Air Bag #2 (High) | 37 | Gr- | Passenger Anchor Pretensioner(High)
38 | G | Passenger Air Bag #2 (Low) | 38 | B | Driver Seat Belt Pretensioner (High)
39 | L | Driver Air Bag (1st Satge (Low)) | 39 | R | Driver Seat Belt Pretensioner (Low)
40 | Br/O | Driver Air Bag (1st Satge (High)) | 40 | Br | Passenger Seat Belt Pretensioner (Low)
41 | Y | Passenger Air Bag #1 (High)v | 41 | L | Passenger Seat Belt Pretensioner(High)
42 | Gr | Passenger Air Bag #1 (Low) | 42 | B | Passenger Seat BaltBuckle Switch (-)
43 | Br | C-CAN (Low) | 43 | W | Driver Pressure Side Impact Sensor (Low)
44 | W | C-CAN (High) | 44 | Br | Driver Pressure Side Impact Sensor (High)

##### Occupant Detecting Sensor (ODS) Repair procedures

Removal 1. Disconnect the battery negative cable, and wait for at least three minutes before beginning work. 2. Remove the front passenger seat assembly. (Refer to the Body group- Seat) 3 ...

##### Brake System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Auto light sensor2. Head lamps3. Lighting switch (Auto)4. Tail lamps5. BCM (Body Control Module) ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Pre-charge Relay Repair procedures

Inspection • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be su ...
Copyright © www.ksoulev.com 2020-2021