- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Charge Door Opener Cover / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Charge Door Opener Cover / Repair procedures

Replacement

1. | Remove the front bumper. (Refer to Front Bumper - "Front Bumper Cover")

2. | Loosen the screws, and then remove the charge door open cover lamp (A).

3. | Disconnect the notification for charge door open cover actuator (A) and charge door opener cover lamp connector (B).

4. | Loosen the screws, and then remove the charge door opener cover assembly (A).

5. | Install in the reverse order of removal.

##### Components and Components Location

Component Location 1. Charge door opener cover ...

##### Hood

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Hood Latch Release Handle Repair procedures

Replacement 1. Using a screwdriver or remover, remove the hood release handle (A). • Use a 6mm hex bit to press the center until the handle easily pulls off the post. 2. Install in the reverse order of removal. • ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: 3-Way Coolant Valve Description and Operation

Description Switches the valve outlet direction through electric signal to change refrigerant flow direction. Directs refrigerant flow towards chiller when heating pump is activated. Directs refrigerant flow towards radiator during normal condition. 1. Towards radiator2. Towards chiller3. I ...
Copyright © www.ksoulev.com 2020-2021