- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Lighting System / High Mounted Stop Lamp Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Lighting System / High Mounted Stop Lamp Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the high mounted stop lamp trim (A).

3. | Detach the high mounted stop lamp (A) from the tailgate after loosening the mounting bolts.

4. | Remove the high mounted stop lamp (C) after disconnecting the connector (B) and hose (A).

Installation

1. | Install the high mounted stop lamp.

2. | Install the high mounted stop lamp trim.

3. | Connect the negative (-) battery terminal.

##### License Plate Lamps Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove the license plate lamp assembly (A). 3. Replace the bulb (B) after removing the license plate lamp (A). Installation ...

##### Luggage Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Using a screwdriver or remover, remove the luggage lamp (A). 3. Remove the luggage lamp (A) after disconnecting the connector (B ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Intake Actuator Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Disconnect the intake actuator connector. 3. Verify that the actuator operates to the recirculation position when 12V is connected to terminal 3 and ground to terminal 7. Verify that the intake actuator operates to the recirculated air posi ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Disc Brake Components and Components Location

Components 1. Guide rod bolt2. Bleed screw3. Caliper carrier4. Caliper body5. Brake pad6. Pad retainer ...
Copyright © www.ksoulev.com 2020-2021