- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Seat Belt / Height Adjust Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Seat Belt / Height Adjust Repair procedures

Replacement

1. | Remove the front seat belt upper anchor. (Refer to Front Seat Belt - "Front Seat Belt Pretensioner")

2. | After loosening the mounting bolts, remove the height adjust (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5kgf.m, 28.9 ~ 39.8 lb-ft)

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Height Adjust Components and Components Location

Component Location 1. Height adjust ...

##### Front Seat Belt Buckle Components and Components Location

Component Location 1. Front seat belt buckle ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components [A/T] 1. Console rear cover assembly2. Floor console assembly3. EPB switch assembly4. Wiring assembly5. Cup Hold assembly6. Console side pad [LH]7. Console side pad [RH]8. Supplement cup hold9. Ashtray10. Floor console mat11. Console storage box12. Hole cover ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Hub / Knuckle Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft) Be careful not to da ...
Copyright © www.ksoulev.com 2020-2021