- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Lighting System / Charge Information Lamp Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Lighting System / Charge Information Lamp Repair procedures

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Using the flat screw driver or remover, remove the crash pad center air vent panel (A).

3. | Disconnect the hazard switch connector (A).

4. | Remove center fascia upper panel (A) after loosening the mounting screws.

5. | Disconnect the charge information lamp connector (A).

6. | Remove the charge information lamp assembly (A) after loosening the mounting screws.

Installation

1. | Install the charge information lamp assembly, center fascia upper panel and crash pad center air vent panel.

2. | Connect the negative (-) battery terminal.

##### Charge Information Lamp Components and Components Location

Components ...

##### Troubleshooting

Troubleshooting SymptomPossible causeRemedyOnly one lamp lights on(All exterior lamps)Bulb burned outReplace bulbSocket, wiring or ground faultyRepair if necessaryHead lamps do not light onBulb b ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Belt Retractor Repair procedures

Replacement • When installing the belt, be careful not to damage the retractor. 1. Remove the rear pillar trim. (Refer to Interior Trim - "Rear Pillar Trim") 2. Loosen the rear seat belt upper anchor (A) mounting bolt. 3. After loosening the ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Management System (BMS) ECU Specifications

Specification ItemSpecificationRemarkC-CAN terminating resistance (?)Approx. 60Combined resistance (BMS ECU-Inverter)C-CAN terminating resistnace (?)Approx. 120BMS ECU resistance ...
Copyright © www.ksoulev.com 2020-2021