- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Door / Rear Door Side Weatherstrip Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door / Rear Door Side Weatherstrip Repair procedures

Replacement

1. | Loosen the rear door checker (B) mounting bolt.
Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m, 12.3 ~ 15.9 lb-ft)

2. | Detach the clips, then remove the rear door side weatherstrip (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Rear Door Belt Inside Weatherstrip Repair procedures

Replacement 1. Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim") 2. Remove the rear door belt inside weatherstrip (A). 3. Install in the reverse order of removal. ...

##### Rear Seat

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Cushion Cover Components and Components Location

Component Location 1. Front seat cushion cover ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Electric Parking Brake (EPB) Description and Operation

Description Description of EPB EPB is an electronic parking brake. Unlike existing parking systems that operate by brake pedals or levers, the EPB system sends a signal to the ECU when the driver operates the EPB switch. The ECU then operates the EPB actuator with motor gears to push the ...
Copyright © www.ksoulev.com 2020-2021