- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / High Voltage Battery Heater Temperature Sensor Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / High Voltage Battery Heater Temperature Sensor Specifications

Specification

Temperature (°C) | Resistance (k?) | Tolerance (%)
-40 | 204.5 | ±4.0
-30 | 117.8 | ±3.5
- 20 | 70.34 | ±3.0
- 10 | 43.43 | ±2.5
0 | 27.63 | ±2.0
10 | 18.07 | ±1.6
20 | 12.11 | ±1.2
30 | 8.303 | ±1.2
40 | 5.813 | ±1.5
50 | 4.149 | ±1.9
60 | 3.013 | ±2.2
70 | 2.225 | ±2.5

##### High Voltage Battery Heater Fuse Repair procedures

Removal Main Relay, Pre Charge Relay, Pre Charge Resistor, Battery Current Sensor, High Voltage Battery Heater Relay and the High Voltage Battery Heater Fuse are in ...

##### High Voltage Battery Heater Temperature Sensor Components and Components Location

Component 1. High Voltage Battery Heater2. High Voltage Battery Heater Relay3. High Voltage Battery Heater Fuse4. High Voltage Battery Heater Temperature Sensor ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Curtain Airbag (CAB) Module Description and Operation

Description Curtain airbags are installed inside the headliner (LH and RH) to protect the driver and passenger from danger when side crash occurs. The SRSCM determines deployment of curtain airbag by using side impact sensor (SIS) signal. Never attempt to measu ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Fuse Description and Operation

High Voltage Battery Heater Fuse It is connected to battery heater relay switch and it cuts off the circuit in case of overcurrent. It is installed in the Power Relay Assembly (PRA).Operation ...
Copyright © www.ksoulev.com 2020-2021